############################################################################
# drivers/input/Make.defs
#
#   Copyright (C) 2011-2012 Gregory Nutt. All rights reserved.
#   Author: Gregory Nutt <gnutt@nuttx.org>
#
# Redistribution and use in source and binary forms, with or without
# modification, are permitted provided that the following conditions
# are met:
#
# 1. Redistributions of source code must retain the above copyright
#    notice, this list of conditions and the following disclaimer.
# 2. Redistributions in binary form must reproduce the above copyright
#    notice, this list of conditions and the following disclaimer in
#    the documentation and/or other materials provided with the
#    distribution.
# 3. Neither the name NuttX nor the names of its contributors may be
#    used to endorse or promote products derived from this software
#    without specific prior written permission.
#
# THIS SOFTWARE IS PROVIDED BY THE COPYRIGHT HOLDERS AND CONTRIBUTORS
# "AS IS" AND ANY EXPRESS OR IMPLIED WARRANTIES, INCLUDING, BUT NOT
# LIMITED TO, THE IMPLIED WARRANTIES OF MERCHANTABILITY AND FITNESS
# FOR A PARTICULAR PURPOSE ARE DISCLAIMED. IN NO EVENT SHALL THE
# COPYRIGHT OWNER OR CONTRIBUTORS BE LIABLE FOR ANY DIRECT, INDIRECT,
# INCIDENTAL, SPECIAL, EXEMPLARY, OR CONSEQUENTIAL DAMAGES (INCLUDING,
# BUT NOT LIMITED TO, PROCUREMENT OF SUBSTITUTE GOODS OR SERVICES; LOSS
# OF USE, DATA, OR PROFITS; OR BUSINESS INTERRUPTION) HOWEVER CAUSED
# AND ON ANY THEORY OF LIABILITY, WHETHER IN CONTRACT, STRICT
# LIABILITY, OR TORT (INCLUDING NEGLIGENCE OR OTHERWISE) ARISING IN
# ANY WAY OUT OF THE USE OF THIS SOFTWARE, EVEN IF ADVISED OF THE
# POSSIBILITY OF SUCH DAMAGE.
#
############################################################################

# Don't build anything if there is no support for input devices

ifeq ($(CONFIG_INPUT),y)

# Include the selected touchscreen drivers

ifeq ($(CONFIG_INPUT_TSC2007),y)
  CSRCS += tsc2007.c
endif

ifeq ($(CONFIG_INPUT_ADS7843E),y)
  CSRCS += ads7843e.c
endif

ifeq ($(CONFIG_INPUT_MAX11802),y)
  CSRCS += max11802.c
endif

ifeq ($(CONFIG_INPUT_MXT),y)
  CSRCS += mxt.c
endif

ifeq ($(CONFIG_INPUT_STMPE811),y)
  CSRCS += stmpe811_base.c
ifneq ($(CONFIG_INPUT_STMPE811_TSC_DISABLE),y)
  CSRCS += stmpe811_tsc.c
endif
ifneq ($(CONFIG_INPUT_STMPE811_GPIO_DISABLE),y)
  CSRCS += stmpe811_gpio.c
endif
ifneq ($(CONFIG_INPUT_STMPE811_ADC_DISABLE),y)
  CSRCS += stmpe811_adc.c
endif
ifneq ($(CONFIG_INPUT_STMPE811_TEMP_DISABLE),y)
  CSRCS += stmpe811_temp.c
endif
endif

ifeq ($(CONFIG_DJOYSTICK),y)
  CSRCS += djoystick.c
endif

ifeq ($(CONFIG_AJOYSTICK),y)
  CSRCS += ajoystick.c
endif

# Include input device driver build support

DEPPATH += --dep-path input
VPATH += :input
CFLAGS += ${shell $(INCDIR) $(INCDIROPT) "$(CC)" $(TOPDIR)$(DELIM)drivers$(DELIM)input}
endif

